( PART NAME=Stirn_Schale_Werkzeuge_Formnest )
( PROGRAM NUMBER=0001 )
( MACHINE=CAMWorks 5AXIS )
( CONTROLLER=GENERIC FANUC )
( MATERIAL=  )
( THICKNESS=25.4 )
( ESTIMATED MACHINE TIME=273 HRS.  38 MIN.  46 SEC. )
( STATION  TOOL TYPE  DIAMETER  CORNER RADIUS  DESCRIPTION               )
( -------  ---------  --------  -------------  -------------------- )
(  006     FACEMILL     100.00                            100MM 9FL FACE MILL)
(  002     ENDMILL      030.00                            30MM CRB 2FL 25 LOC  )
(  004     ENDMILL      009.00                            9MM CRB 2FL 15 LOC  )
(  009     ENDMILL      012.00                            12MM CRB 2FL 19 LOC  )
(  012     ENDMILL      002.00                            2MM CRB 2FL 12 LOC  )
(  007     COUNTER SINK 008.00                            8MM HSS 60DEG COUNTERSINK)
(  014     COUNTER SINK 003.00                            3MM HSS 60DEG COUNTERSINK)
(  016     LOLLIPOP        003.00                         3MM CRB 2FL LOLLIPOP)
(  008     LOLLIPOP        003.30                         3.3MM CRB 2FL LOLLIPOP)
(  013     LOLLIPOP        002.20                         2.2MM CRB 2FL LOLLIPOP)
(  011     ENDMILL      004.00                            4MM CRB 2FL 14 LOC  )
(  010     ENDMILL      001.00                            1MM CRB 2FL 14 LOC  )
(  005     COUNTER SINK 003.00                            3MM HSS 60DEG COUNTERSINK)
(  017     HOGNOSE      004.00      001.00            4mm CRB 4FL HGN 1R 4MM LOC)
(  001     HOGNOSE      004.00      002.00            4MM CRB 2FL 50 LOC)
(  015     LOLLIPOP        000.50                         0.5MM CRB 2FL LOLLIPOP)
(  003     ENDMILL      000.20                            .2MM CRB 2FL 15 LOC  )
